{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["Cross","GB","Briscon","King","Dottie","Thiel","Sturgeon","Ideal","Wireline","Viking","Arrow"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cross","index":0,"n_rows":2,"n_cols":8,"rows_kept":2,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["Staple Cross"]
["GB SKU","Briscon","King","Viking","Dottie","Thiel","Sturgeon","Exact / Close"]

{"sheet":"GB","index":1,"n_rows":39,"n_cols":11,"rows_kept":39,"flags":["formulas_cached_only"]}
["GB SKU","UPC","Wire Size","Dimensions","Color","Material / Use","ALT UPC AND/OR NOTES","Brand Group","Brand","COUNTRY OF ORIGIN","Cable Count"]
["MS-150","032076651503","#12 & 14","1/2\"x1\"","NA","2 Cond / Metal",0,"GB","Gardner Bender","US","One"]
["MS-175","032076651756","#10 & 12","9/16\"x1-1/4\"","NA","3 Cond / Metal",0,"GB","Gardner Bender","US","One"]
["MSI-150","032076894481","12/2, 14/2, 10/2","1/2\"","Blue","Insulated / Metal",0,"GB","Gardner Bender","US","One"]
["MSI-75","032076912017","14/3, 12/3, 10/3","9/16\"","Blue","Insulated / Metal",0,"GB","Gardner Bender","US","One"]
["MSI-50XL",null,"14/2, 12/3, 10/3","1-1/2\"x1/2\"","Red","Double Stack / Insulated / Metal",{"$nulls":3},"US","Two"]
["GSE-310","032076003098","SEU #6/3 w/g","13/16\"x1-3/8\"","NA","Svc Ent / Metal",0,"GB","Gardner Bender","US","One"]
["GSE-410","032076003104","4/3, 2/3 SE","1-1/16\"x1-7/16\"","NA","Svc Ent / Metal",0,"GB","Gardner Bender","US","One"]
["GSE-710","032076032692","4/0 SE","1-5/8\"x2-1/8\"","NA","Svc Ent / Metal",0,"GB","Gardner Bender","US","One"]
["PS-150","032076661502","12/2 & 14/2 ","1/2\"","White","Plastic / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PS-175","032076661755","14/2, 12/2, 10/2","3/4\"","White","Plastic / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["MCS-100W","032076057657","Multi ","NA","Red","SnapShot / Metal",0,"GB","Gardner Bender","CN","Multi"]
["PS-50M","032076914356","14/2, 12/2, 10/2","1/2\"","White","Masonry / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PS-75M","032076914349","14/3, 12/3, 10/3","3/4\"","White","Masonry / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["GSE-115","032076912109","#6 SEU","3/4\"","Gray","Svc Ent / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["GSE-215","032076912093","#2 SEU","15/16\"","Gray","Svc Ent / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["GSE-314","032076912086","#2 SER","31/32\"","Gray","Svc Ent / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["GSE-402","032076011970","#4/0 SEU","1-1/2\"","Gray","Svc Ent / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["GSE-515","032076912079","#6 SER","45/64\"","Gray","Svc Ent / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PSB-165","032076893699","RG-59, RG-6","1/4\"","Black","Coax / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PSW-165","032076894184","RG-59, RG-6","1/4\"","White","Coax / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PCC-1525","032076047436","RG-59, RG-6","1/4\"","Black","Coax / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PSG-15","032076003012","RG-59, RG-6","1/4\"","Gray","Coax / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PSG-50","032076912611","RG-59, RG-6, RG-8","7/16\"","Gray","Coax / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PR-50","032076032678","RG-59, RG-6, RG-8","7/16\"","White","Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PMB-1525","032076002992","Low Voltage","1/8\"","Black","Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PMW-100B","032076003234","Low Voltage","3/16\"","White","Zinc Plated","Substitute Item PMW-100B","GB","Gardner Bender","US","One"]
["PSB-1600T","032076912529","Low Voltage","3/16\"","Black","Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PSW-1600T","032076912574","Low Voltage","3/16\"","White","Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PMC-1525WT","032076912499","Low Voltage","3/16\"","White","Masonry / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PTP-100","032076912048","Cat3, Cat5","1/4\"","Blue","Data / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PTP-100M","032076914387","Cat3, Cat5","1/4\"","Blue","Data / Masonry / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PCS-100","032076032685","RG-59, RG-6","1/4\"","Black","Coax / Masonry",0,"GB","Gardner Bender","US","One"]
["PSR-25","032076047030","RG-59, RG-6","1/4\"","Black","Coax / Roofing / Zinc Plated",0,"GB","Gardner Bender","US","One"]
["PDS-1525BT","032076912482","RG-59, RG-6","1/4\"","Black","Coax / Zinc Plated / Double",0,"GB","Gardner Bender","US","Two"]
["PDC-1525BT","032076912475","RG-59, RG-6","1/4\"","Black","Coax / Masonry / Metal / Double",0,"GB","Gardner Bender","US","Two"]
["MSB-1540","032076154004","Low Voltage","1/8\"","Brown","Insulated / Metal",0,"GB","Gardner Bender","CN","One"]
["MSW-1540","032076154011","Low Voltage","1/8\"","White","Insulated / Metal",0,"GB","Gardner Bender","CN","One"]
["PWS-1525","032076002695","Cat5","7/8\"x3/16\"x1/4\"","White","Kwik Mount / Metal / Double",0,"GB","Gardner Bender","US","Two"]

{"sheet":"Briscon","index":2,"n_rows":81,"n_cols":10,"rows_kept":81,"merged":[[1,2,5,2],[1,5,5,5],[1,6,5,6],[1,7,5,7],[1,8,5,8],[1,9,5,9],[6,2,11,2],[6,5,11,5],[6,6,11,6],[6,7,11,7],[6,8,11,8],[6,9,11,9],[12,2,16,2],[12,5,16,5],[12,6,16,6],[12,7,16,7],[12,8,16,8],[12,9,16,9],[17,2,20,2],[17,5,20,5],[17,6,20,6],[17,7,20,7],[17,8,20,8],[17,9,20,9],[21,2,24,2],[21,5,24,5],[21,6,24,6],[21,7,24,7],[21,8,24,8],[21,9,24,9],[25,2,27,2],[25,5,27,5],[25,6,27,6],[25,7,27,7],[25,8,27,8],[25,9,27,9],[28,2,30,2],[28,5,30,5],[28,6,30,6],[28,7,30,7],[28,8,30,8],[28,9,30,9],[31,2,33,2],[31,5,33,5],[31,6,33,6],[31,7,33,7],[31,8,33,8],[31,9,33,9],[35,2,36,2],[35,5,36,5],[35,6,36,6],[35,7,36,7],[35,8,36,8],[35,9,36,9],[57,2,65,2],[57,5,65,5],[57,8,65,8],[57,9,65,9],[66,2,71,2],[66,5,71,5],[66,8,71,8],[66,9,71,9],[72,2,78,2],[72,8,78,8],[72,9,78,9],[79,2,80,2],[79,5,80,5],[79,8,80,8],[79,9,80,9]],"flags":["formulas_cached_only"]}
["GB","Cross","Group","UPC #","QTY","Material","Width","Length","UL","Discription"]
["NA","SN 40 500","SN 40",72403,500,"Low Carbon Steel","1/2\" Wide","1\" Long","NO","Armored Cable 14/2 And 14/3, Metal Clad 14/2 And 14/3, Non-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 And 12/2"]
["NA","SN 40 5M",null,72405,"5000 BUCKET"]
["NA","SN 40 J 1500",null,72404,"1500 JAR"]
["NA","SN 40 10M",null,72407,"10000 BUCKET"]
["NA","SN 40 15M",null,72409,"15000 BUCKET "]
["MS-150","SN 40 B 100","SN 40 B",71966,100,"Zinc Plated Low Carbon Steel","1/2\" Wide","1\" Long","YES","Armored Cable 14/2 And 14/3, Metal Clad 14/2 And 14/3, Non-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 And 12/2"]
["NA","SN 40 B 500",null,71968,500]
["NA","SN 40 BJ 1500",null,71969,"1500 JAR"]
["NA","SN 40 B 5M",null,71970,"5000 BUCKET"]
["NA","SN 40 B 10M ",null,71975,"10000 BUCKET"]
["NA","SN 40 B 15M ",null,71977,"15000 BUCKET"]
["MSI-150","SN 40 IB 100","SN 40 IB",71981,100,"Zinc Plated Low Carbon Steel","1/2\" Wide","1\" Long","YES","LDPE Blue Plastic Insulator, Armored Cable 14/2 And 14/3, Metal Clad 14/2 And 14/3, Non-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 And 12/2"]
["NA","SN 40 IB 500",null,71984,500]
["NA","SN 40 IBJ 500",null,71983,"500 JAR"]
["NA","SN 40 IB 2500",null,71980,2500]
["NA","SN 40 IB 5M",null,71985,5000]
["NA","SN 100 500","SN 100",72993,500,"Low Carbon Steel","9/16\" Wide","1-1/4\" Long","NO","Armored Cable 14/2 through 10/3, Metal Clad 14/2 through 10/3, Non-metallic Sheathed 12/3 through 10/3, Underground Feeder 14/3 And 12/3"]
["NA","SN 100 J 1M ",null,72983,"1000 JAR"]
["NA","SN 100 5M ",null,72985,"5000 BUCKET"]
["NA","SN 100 10M",null,72997,"10000 BUCKET"]
["MS-175","SN 100 B 100","SN 100 B",71986,100,"Zinc Plated Low Carbon Steel","9/16\" Wide","1-1/4\" Long","YES","Armored Cable 14/2 Through 10/3, Metal Clad 14/2 Through 10/3, Non-metallic Sheathed 12/3 through 10/3, Underground Feeder 14/3 And 12/3"]
["NA","SN 100 B 500",null,71995,500]
["NA","SN 100 BJ 1M",null,71987,"1000 JAR"]
["NA","SN 100 B 4M ",null,71990,"4000 BUCKET"]
["NA","SN 100 IB 100","SN 100 IB",72610,100,"Zinc Plated Low Carbon Steel","9/16\" Wide","1-1/4\" Long","YES","Armored Cable 14/2 through 10/3, \nMetal Clad 14/2 through 10/3, Non-metallic Sheathed 12/3 through 10/3, Underground Feeder 14/3 And 12/3"]
["NA","SN 100 IB 250",null,72613,250]
["NA","SN 100 IB 3M",null,72615,"3000 BUCKET"]
["NA","SN 150 B 100","SN 150 B",75025,100,"Zinc Plated Low Carbon Steel","1/2\" Wide","1-1/2\" Long","YES","One Cable\n Non-metallic Sheathed 14/2 Through 10/3\nUnderground Feeder 14/2 And 12/2\nTwo Cables\nNon-metallic Sheathed 14/2 Through 12/3\nUnderground Feeder 14/2 And 12/2\n"]
["NA","SN 150 B 500",null,75030,500]
["NA","SN 150 B 2500",null,75035,"2500 BUCKET"]
["NA","SN 150 IB 100","SN 150 IB",75027,100,"Zinc Plated Low Carbon Steel","1/2\" Wide","1-1/2\" Long","YES","One Cable\n Non-metallic Sheathed 14/2 Through 10/3\nUnderground Feeder 14/2 And 12/2\nTwo Cables\nNon-metallic Sheathed 14/2 Through 12/3\nUnderground Feeder 14/2 And 12/2\n"]
["NA","SN 150 IB 250",null,75028,250]
["NA","SN 150 IB 3M",null,75026,"3000 BUCKET"]
["NA","SN 300 B 100","SN 300 B",73302,100,"Zinc Plated Low Carbon Steel","13/16\" Wide","1-3/8\" Long","YES","Armored Cable 8/3, Metal Clad 8/3, SE Cable 8/2 Through 6/3\nNon metallic Sheathed 8/3 Through 6/3, Underground Feeder 10/3"]
["NA","SN 300 IB 100","SN 300 IB",73305,100,"Zinc Plated Low Carbon Steel","13/16\" Wide","1-3/8\" Long","YES","Armored Cable 8/3, Metal Clad 8/3, SE Cable 8/2 Through 6/3\nNon metallic Sheathed 8/3 Through 6/3, Underground Feeder 10/3"]
["NA","SN 300 IBJ 175",null,75312,175]
["GSE-310","SN 350 B 100","SN 350 B ",73350,100,"Zinc Plated Low Carbon Steel","1-1/16\" Wide","1-7/16\" Long","YES","se Cable 4/3 SEU Through 2/3 SER"]
["NA","SN 350 IB 50","SN 350 IB",73356,50,"Zinc Plated Low Carbon Steel","1-1/16\" Wide","1-7/16\" Long","NO","SE Cable 4/3 SEU Through 2/3 SER"]
["NA","SN 400 B 100","SN 400 B",73400,100,"Zinc Plated Low Carbon Steel","1-11/32\" Wide","1-7/8\" Long","YES","SE Cable 3 No. 2/0 SEU, SE Cable 3 No. 2/0 SER"]
["NA","SN 450 B 100","SN 450 B",73450,100,"Zinc Plated Low Carbon Steel","1-3/16\" Wide","2-1/4\" Long","YES","Armored Cable 2/3, SE Cable 3 No. 1/0 SER, Underground Feeder 6/3"]
["NA","SN 500 B 100","SN 500 B",73500,100,"Zinc Plated Low Carbon Steel","1-5/8\" Wide","2-1/8\" Long","YES","SE Cable 3 No. 4/0 SEU, SE Cable 3 No. 4/0 SER"]
["NA","SN 600 100","SN 600",74600,100,"Zinc Plated Low Carbon Steel","1-1/16\" Wide","2-1/16\" Long","NO","4/3 SER Cable, 2/3 SER Cable, 3/4\" EMT, 1/2 Greenfield"]
["NA","SN 700 100","SN 700",74700,100,"Zinc Plated Low Carbon Steel","1-11/32\" Wide","2-11/32\" Long","NO","2/0 SER Cable, 1\" EMT, 1\" Greenfield"]
["NA","SN 800 100","SN 800",74800,100,"Zinc Plated Low Carbon Steel","1-3/16\" Wide","2-3/16\" Long","NO","2/3 BX, 1\" EMT, 1\" Greenfield, 2/3 SER Cable"]
["NA","SN 900 100","SN 900",74900,100,"Zinc Plated Low Carbon Steel","1-5/8\" Wide","2-5/8\" Long","NO","4/0 SER Cable, 1\" And 1-1/4\" EMT,\nLarge BX NM, Greenfield"]
["NA","SN 1000 20 ","SN 1000",75000,20,"Zinc Plated Low Carbon Steel","1-1/4\" Wide","2-3/4\" Long","NO","Large Metal Clad And Non-metallic Cable Greenfield"]
["NA","SN 40 B SS 100 ","SN 40 B SS",10035,100,"Stainless Steel","1/2\" Wide","1\" Long","YES","Armored Cable 14/2 And 14/3, Metal Clad 14/2 And 14/3, \nNon-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 And 12/2"]
["NA","SN 40 IB SS 100","SN 40 IB SS",10030,100,"Stainless Steel, LDPE Blue Plastic Insulator","1/2\" Wide","1\" Long","YES","Armored Cable 14/2 And 14/3, Metal Clad 14/2 And 14/3, \nNon-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 And 12/2"]
["NA","SN 100 B SS 100","SN 100 B SS",71997,100,"Stainless Steel","9/16\" Wide","1-1/4\" Long","YES","Armored Cable 14/2 through 10/3, Metal Clad 14/2 through 10/3, \nNon-metallic Sheathed 12/3 through 10/3, Underground Feeder 14/3 And 12/3"]
["NA","SN 100 IB SS 100","SN 100 IB SS",72617,100,"Stainless Steel, LDPE Yellow Plastic Insulator","9/16\" Wide","1-1/4\" Long","NO","Armored Cable 14/2 Through 10/3, Metal Clad 14/2 Through 10/3, \nNon-metallic Sheathed 14/2 Through 10/3, Underground Feeder 14/2 Through 12/3,\n"]
["NA","SN 150 B SS 100","SN 150 B SS",75041,100,"Stainless Steel","1/2\" Wide","1-1/2\" Long","YES ","One Cable\n Non-metallic Sheathed 14/2 Through 10/3\nUnderground Feeder 14/2 And 12/2\nTwo Cables\nNon-metallic Sheathed 14/2 Through 12/3\nUnderground Feeder 14/2 And 12/2\n"]
["NA","SN 150 IB SS 100","SN 150 IB SS",75031,100,"Stainless Steel, LDPE Red Plastic Insulator","1/2\" Wide","1-1/2\" Long","YES","One Cable\n Non-metallic Sheathed 14/2 Through 10/3\nUnderground Feeder 14/2 And 12/2\nTwo Cables\nNon-metallic Sheathed 14/2 Through 12/3\nUnderground Feeder 14/2 And 12/2\n"]
["NA","SN 300 IB SS 100","SN 300 B SS",73303,100,"Stainless Steel","13/16\" Wide","1-3/8\" Long","YES","Armored Cable 8/3, Metal Clad 8/3, SE Cable 8/2 Through 6/3\nNon metallic Sheathed 8/3 Through 6/3, Underground Feeder 10/3"]
["NA","SN 200 IB SS 100","SN 300 IB SS",73308,100,"Stainless Steel LDPE Grey Plastic Insulator","13/16\" Wide","1-3/8\" Long","YES","Armored Cable 8/3, Metal Clad 8/3, SE Cable 8/2 Through 6/3\nNon metallic Sheathed 8/3 Through 6/3, Underground Feeder 10/3"]
["NA","SN 250 B SS 100","SN 350 B SS",73353,100,"Stainless Steel","1-1/16\" Wide","1-7/16\" Long","YES","se Cable 4/3 SEU Through 2/3 SER"]
["NA","SN 350 IB SS 50","SN 350 IB SS",73354,50,"Stainless Steel LDPE Grey Plastic Insulator","1-1/16\" Wide","1-7/16\" Long","NO","se Cable 4/3 SEU Through 2/3 SER"]
["PS-150","PS 50 100","Plastic Staples",72512,100,"Zinc Plated with Plastic Saddle","1/2\" Wide","1-1/4\" Long","NO","Plastic Saddles, Zinc Plated Nails \nResist Rust and Corrosion"]
["PS-175","PS 75 100",null,72517,100,null,"3/4\" Wide","1-1/4\" Long"]
["GSE-170","PS 300 100",null,411753,100,null,"3/4\" Wide","1-3/4\" Long"]
["GSE-515","PS 300 R 100",null,411740,100,null,"3/4\" Wide","1-3/4\" Long"]
["NA","PS 350 50",null,41745,50,null,"1\" Wide","1-3/4\" Long"]
["GSE-330","PS 350 R 50",null,41750,50,null,"1\" Wide","2\" Long"]
["NA","PS 400 R 50",null,41753,50,null,"1-1/4\" Wide","2-1/2\" Long"]
["GSE-402","PS 500 50",null,41755,50,null,"1-1/2\" Wide","2\" Long"]
["NA","PS 500 R 25",null,41760,25,null,"1-1/2\" Wide","2\" Long"]
["PSG-100","CX 90 100","Coaxial Staples",75050,100,"Zinc Plated","1/2\" Wide","1\" Long","NO","Use with RG-59, RG-6, Category 5 and Other Cables Up to 1/4\"\nZinc Plated Nail and Staple Resist Rust and Corrosion"]
["NA","CX 90 J 500",null,75056,"500 JAR",null,"1/2\" Wide","1\" Long"]
["PSB-100","PS 90 B 100",null,72522,100,null,"1/4\" Wide","1\" Long"]
["NA","PS 90 BJ 500",null,72524,"500 JAR",null,"1/4\" Wide","1\" Long"]
["PSW-100","PS 90 W 100",null,72523,100,null,"1/4\" Wide","1\" Long"]
["NA","PS 90 WJ 500",null,72525,"500 JAR",null,"1/4\" Wide","1\" Long"]
["NA","#1 COPPER 100","Low Voltage\nInsulated Staples",71137,100,null,"3/16\" Wide","1/2\" Long","NO","Low Voltage Staples for use with bell speaker, thermostat and telephone wire . \nAll Sizes: Standard Package 1000 staples; approximate weight 2 pounds/1000"]
["NA","#3 COPPER 100",null,71337,100,null,"3/16\" Wide","3/4\" Long"]
["MSB-1540","#5 BROWN 40",null,71512,40,null,"1/4\" Wide","5/8\" Long"]
["NA","#5 COPPER 100",null,71537,100,null,"1/4\" Wide","5/8\" Long"]
["MSW-1540","#5 WHITE 40",null,71516,40,null,"1/4\" Wide","5/8\" Long"]
["NA","#6 COPPER 100",null,71637,100,null,"1/4\" Wide","3/4\" Long"]
["NA","#7 COPPER 100",null,71737,100,null,"1/4\" Wide","7/8\" Long"]
["PSW-160","PS 80 W 100","Low Voltage \nPlatstic Staples",72541,100,"Zinc Plated","3/16\" Wide","1\" Long","NO","Low Volatage Staples for use with bell, speaker, thermostat and telephone wire. \nZinc plated nail resists rust and corrosion."]
["PSB-160","PS 80 B 100",null,72531,100,null,"3/16\" Wide","1\" Long"]

{"sheet":"King","index":3,"n_rows":72,"n_cols":3,"rows_kept":72,"merged":[[1,0,1,1],[1,2,7,2],[8,0,8,1],[8,2,14,2],[15,0,15,1],[15,2,21,2],[22,0,22,1],[28,0,28,1],[28,2,31,2],[32,0,32,1],[32,2,35,2],[36,0,36,1],[36,2,43,2],[44,0,44,1],[44,2,51,2],[52,0,52,1],[57,0,57,1],[58,2,61,2],[62,0,62,1],[63,2,67,2],[68,0,68,1]],"flags":["formulas_cached_only"]}
["GB","King","Description"]
[null,null,"1/2\" x 1\" For NM-B #12-14 Wire (Metal)"]
["NA","03421"]
["NA","03422"]
["NA","03423"]
["NA","03424"]
["MS-550","03457"]
["MS-150","03458"]
[null,null,"9/16\" x 1-1/4\" For NM-B #10-12-14 3 Cond BX - MC (Metal)"]
["MS-975B","03425"]
["MS-975B","03426"]
["MS-975B","03427"]
["MS-975B","03428"]
["MS-975B","03460"]
["MS-975B","03461"]
[null,null,"9/16\" x 1\" For #10-12-14 NM-B (Plastic Insulated)"]
["MSI-75","06021"]
["MSI-75","06022"]
["MSI-75","06023"]
["MSI-75","06024"]
["MSI-75","06025"]
["MSI-75","06026"]
[null,null,"Large - Zinc Plated"]
["GSE-310","09021","1-3/8\" x 12/16\" (6-3 SE, BX Range Cords)"]
["NA","09022","1-7/16\" x 1-1/16\" (4-3 SER, 2-3 SE, 3/4\" EMT)"]
["NA","09023","1-7/8\" x 1-11/32\" (2-0 SE, 1\" EMT)"]
["NA","09024","2-1/4\" x 1-3/16\" (2-3 BX, 1\" EMT, 22-3 SET, 1\" Greenfield)"]
["GSE-710","09025","2-1/8\" x 1-5/8\" ( 2-0 SE, Greenfield, Tubing)"]
[null,null,"1/2\" x 1\" For #12-14 NM-B (Stainless Steel)"]
["NA","09015"]
["NA","09016"]
["NA","09017"]
[null,null,"9/16\" x 1\" For #10-12-14 NM-B (Stainless Steel)"]
["NA","09018"]
["NA","09019"]
["NA","09020"]
[null,null,"1/2\" x 1\" For NM-B #12-14 Wire (Rigid Metal)"]
["MS-550","03442"]
["MS-150","03443"]
["NA","03480"]
["NA","03481"]
["NA","03482"]
["NA","03483"]
["NA","09013"]
[null,null,"9/16\" x 1-1/4\" For NM-B #10-12-14 3 Cond BX - MC (Metal)"]
["MS-575","03446"]
["MS-175","03447"]
["NA","03484"]
["NA","03485"]
["NA","03486"]
["NA","03487"]
["NA","09014"]
[null,null,"Service Cable Staples"]
["NA","07049","3/4\" x 1-3/8\""]
["NA","07050","7/8\" x 1-3/8\""]
["NA","07053","3/4\" x 1-3/8\""]
["NA","07054","7/8\" x 1-3/8\""]
[null,null,"Multi-Stack Staples"]
["NA","05000","9/16\" x 1-1/2\" For type NM: One Wire: 14/2 through 10/3 Two Wire: 14/2 through 12/3 For Type UF: One Wire: 14/2 through 12/2 Two Wire: 14/2 through 12/2"]
["NA","02500"]
["NA","01250"]
["NA","00100"]
[null,null,"Insulated Multi-Stack Staples"]
["NA","06028","9/16\" x 1-1/2\" For type NM: One Wire: 14/2 through 10/3 Two Wire: 14/2 through 12/3 For Type UF: One Wire: 14/2 through 12/2 Two Wire: 14/2 through 12/2"]
["NA","06029"]
["NA","06030"]
["NA","06031"]
["NA","06032"]
[null,null,"Ground Wire Staples"]
["NA","00088","1/4\" x 1-3/8\" "]
["NA","00094","3/8\" x 1-5/8\""]
["NA","00011","1/2\" x 2\""]

{"sheet":"Dottie","index":4,"n_rows":29,"n_cols":8,"rows_kept":29,"merged":[[1,2,4,2],[5,2,8,2],[9,2,10,2],[11,2,13,2],[14,2,16,2],[17,2,18,2],[19,2,21,2],[22,2,24,2],[25,2,26,2],[27,2,28,2]],"flags":["formulas_cached_only"]}
["GB","Cross","Discription","UPC","Size","AWG","Packing","Unit"]
["MS-150","RX501","Staples PC 5020, 5025 1/2” - 2 Conductor (#12 & #14) Romex® and other type NM Cable - PC 5020",30710,"14-2, 12-2 1/2 x 1\"","12 GA","100 5000 "," 0.57# M"]
["MS-550","RX505",null,30715," 14-2, 12-2 1/2 x 1\" ","12 GA","500 5000","2.75# M"]
["MS-950B","RX50B",null,30720," 14-2, 12-2 1/2 x 1\" ","12 GA","5000 5000","28.12# M"]
["MS-950BU","RX503P",null,30725," 14-2, 12-2 1/2 x 1\" ","12 GA","10000 10000(Pail) ","56.60# M"]
["MS-175","BX1001","9/16\" - 3 Conductor (#10, #12 & #14) Romex®, BX, MC and other Cable - PC 5020",27010," 14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","100 5000 ","0.69# M"]
["MS-575","BX1005 ",null,27015," 14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","500 5000","3.38# M"]
["MS-975B","BX100B",null,27020," 14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","5000 5000","34.50# M"]
["NA","BX3P",null,27025," 14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","7500 7500(Pail)","51.64# M"]
["NA","SEU63","SEU - PC 5025",27130,"6/3 SEU Cable 13/16 x 1-3/8\"","12 GA","100 1000","1.09# M"]
["NA","SEU43",null,27135,"4/3 & 2/3 SEU Cable1-1/8 x 1-1/2\"","12 GA","100 1000","1.30# M"]
["NA","RXG501","Staples - Electro Galvanized PC 5022, 5024 1/2” - 2 Conductor (#12 & #14) Romex® and other type NM Cable - PC 5022",10530,"14-2, 12-2, 10-2 1/2 x 1\"","12 GA","100 5000","0.60# M"]
["NA","RXG505",null,10531,"14-2, 12-2, 10-2 1/2 x 1\"","12 GA","500 5000","2.85# M"]
["NA","RXG503P",null,10532,"14-2, 12-2, 10-2 1/2 x 1\"","12 GA","10000 10000(Pail) ","59.50# M"]
["NA","BXG1001","9/16\" - 3 Conductor (#10, #12 & #14) Romex®, BX, MC and other Cable - PC 5022",10533,"14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","100 5000","0.70# M"]
["NA","BXG1005",null,10534,"14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","500 5000","3.50# M"]
["NA","BXG3P",null,10535,"14-3, 12-3, 10-3 9/16 x 1-3/16\"","12 GA","7500 7500(Pail)","52.50# M"]
["NA","SEU63G","SEU - PC 5024",27131,"6/3 SEU Cable 13/16 x 1-3/8\" ","12 GA","100 1000","1.09# M"]
["NA","SEU43G",null,27136,"4/3 & 2/3 SEU Cable1-1/8 x 1-1/2\"","12 GA","100 1000","1.32# M"]
["PS-150","PLX501","Staples - Plastic Insulated PC 5026 1/2” - 2 Conductor (#12 & #14) Romex® and other type NM Cable",27140,"14-2, 12-2 1/2\" ","White","100 5000","0.57# M"]
["PS-550","PLX505",null,27142,"14-2, 12-2 1/2\" ","White","500 5000","2.44# M"]
["PS-750B","PLX50P",null,27144,"14-2, 12-2 1/2\" ","White","4000 4000(Pail)","22.80# M"]
["NA","PLX751","9/16\" - 3 Conductor (#10, #12 & #14) Romex®, BX, MC and other Cable",27146,"14-3, 12-3, 10-3 3/4\"","White","100 5000","0.62# M"]
["NA","PLX755",null,27148,"14-3, 12-3, 10-3 3/4\"","White","500 5000","2.53# M"]
["NA","PLX75P",null,27150,"14-3, 12-3, 10-3 3/4\"","White","3000 3000(Pail)"," 15.60# M"]
["PSW-100","PLX250W","Co-Axial Straps (Use Co-Axial RG-6 & RG-59U)",10523,"1/4\"","White","500 3000","1.16# M"]
["PSB-100","PLX250B",null,10539,"1/4\"","Black","500 3000","1.16# M"]
["PSW-160","PLX18W","Bell, Telephone & Thermostat Wire Straps",10540,"1/4 x 1/8\"","White","500 3000","1.08# M"]
["PSB+160","PLX18B",null,10541,"1/4 x 1/8\"","Black","500 3000","1.08# M"]

{"sheet":"Thiel","index":5,"n_rows":20,"n_cols":8,"rows_kept":20,"merged":[[1,0,4,0],[1,2,4,2],[5,0,7,0],[5,2,7,2],[8,0,11,0],[8,2,11,2],[12,0,15,0],[12,2,15,2],[16,2,17,2],[18,2,19,2]],"flags":["formulas_cached_only"]}
["GB","Cross","Discription","UPC","Size","AWG","Box","Case"]
["MSI-100","1100-IN-1","1100-IN 1\" L X 1/2\" W - Insulated staple, high-impact hot-melt PVC bonded to the upper portion of the staple. Dielectric rating per ETL Test 525777: 250 volts per mil., 10 mils minimum coverage on the area of impact and cable contact. Available in blue, orange, and yellow. APPLICATION: Romex (NMC) 2-Conductor 14 & 12, With or Without Ground. SPECIFICATION: 12 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1\" L X 1/2\" W","12 GA",100,5000]
[null,"1100-IN-5",null,"NA","1\" L X 1/2\" W","12 GA",500,5000]
[null,"1100-IN-PB5M",null,"NA","1\" L X 1/2\" W","12 GA","Bucket",5000]
[null,"1100-IN-PB10M",null,"NA","1\" L X 1/2\" W","12 GA","Bucket",10000]
["MSI-75","1125-IN-1","1125-IN 1-1/4\" L X 9/16\" W - Insulated staple, high-impact hot-melt PVC bonded to the upper portion of the staple. Dielectric rating per ETL Test 525777: 250 volts per mil., 10 mils minimum coverage on the area of impact and cable contact. Available in blue, orange, and yellow. APPLICATION: BX or Romex 3-Conductor 14, 12 & 10 WG or 2 Stacked Oval Romex 14 & 12 WG. SPECIFICATION: 12 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1-1/4\" L X 9/16\" W","12 GA",100,5000]
[null,"1125-IN-5",null,"NA","1-1/4\" L X 9/16\" W","12 GA",500,5000]
[null,"1125-IN-PB5M",null,"NA","1-1/4\" L X 9/16\" W","12 GA","Bucket",5000]
["MS-150","1100-1","1100 1\" L X 1/2\" W Non-Insulated Staples APPLICATION: Romex (NMC) 2-Conductor 14 & 12 WG, With or Without Ground SPECIFICATION:\n12 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1\" L X 1/2\" W","12 GA",100,10000]
[null,"1100-5",null,"NA","1\" L X 1/2\" W","12 GA",500,10000]
[null,"1100-PB5M",null,"NA","1\" L X 1/2\" W","12 GA","Bucket",5000]
[null,"1100-PB10M",null,"NA","1\" L X 1/2\" W","12 GA","Bucket",10000]
["MS-175","1125-1","1125 1-1/4\" L X 9/16\" W Non-Insulated Staples APPLICATION: BX or Romex 3-Conductor 14, 12 & 10 WG (A) or 2 Stacked Oval Romex - 14 & 12 WG (B) SPECIFICATION: 12 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1-1/4\" L X 9/16\"","12 GA",100,10000]
[null,"1125-5",null,"NA","1-1/4\" L X 9/16\"","12 GA",500,10000]
[null,"1125-PB5M",null,"NA","1-1/4\" L X 9/16\"","12 GA","Bucket",5000]
[null,"1125-PB8M",null,"NA","1-1/4\" L X 9/16\"","12 GA","Bucket",8000]
["NA","1150-1","1150 1-5/16\" L X 3/4\" W - Service Entrance Staples APPLICATION: Service Entrance SEU - 3/5 SPECIFICATION: 10 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1-5/16\" L X 3/4\" W","10 GA",100,5000]
["NA","1150-PB4M",null,"NA","1-5/16\" L X 3/4\" W","10 GA","Bucket",4000]
["NA","1175-1","1175 1-9/16\" L X 1-1/16\" W - Service Entrance Staples APPLICATION: Service Entrance SEU - 2/3 SPECIFICATION: 11 Gauge Carbon Steel, Tumble Deburred and Burnished, Rust Inhibitor Applied During Tumbling.","NA","1-9/16\" L X 1-1/16\" W","11 GA",100,2000]
["NA","1175-PB2.5M",null,"NA","1-9/16\" L X 1-1/16\" W","11 GA","Bucket",2500]

{"sheet":"Sturgeon","index":6,"n_rows":97,"n_cols":6,"rows_kept":97,"merged":[[2,2,8,2],[10,2,11,2],[12,2,13,2],[14,2,15,2],[17,2,22,2],[45,2,48,2],[88,2,90,2],[91,2,93,2],[94,2,96,2]],"flags":["formulas_cached_only"]}
["GB","Cross","Discription","Size","Color","Pack"]
[null,null,"Straps for Nonmetallic-Sheathed (NM) and Underground Feeder (UF) Cable"]
["PS-150Z","RA-1477P"," - 1/2” STRAP FOR 2, 3, AND 4 WIRE NM CABLE UP TO 10/3, UF CABLE UP TO 12/2, AND OTHER CABLE UP TO .500” WIDE","1/2”","White","Bag 100"]
["PS-150","RA-1577",null,"1/2”","White","Box 100"]
["PS-750B","RA-1580",null,"1/2”","White","Bulk 5000"]
["PS-750B","RA-1581",null,"1/2”","White","Pail 1000"]
["PS-750B","RA-1582",null,"1/2”","White","Pail 2000"]
["PS-750B","RA-1585",null,"1/2”","White","Pail 5000"]
["NA","RA-1588 or RA1588UV",null,"1/2”","Black","Bag 5000"]
[null,null,"1/2” STACKER STRAPS FOR SECURING MORE THAN ONE NM OR UF CABLE - Secure combinations of NM and UF Cable to narrow structural members with one strap. Color coded for easy identification. "]
["MSI-50XL","RA-1588/2","For two 2 wire NM or UF Cables stacked up to 3/8” high. "," 1/2”","Tan","Box 50"]
["MSI-50XL","RA-1582/2",null," 1/2”","Tan","Pail 1000"]
["NA","RA-1588/3","For three 2 wire cables or combinations of 2, 3, and 4 wire cables stacked up to 1/2” high. "," 1/2”","Gray","Box 50"]
["NA","RA-1582/3",null," 1/2”","Gray","Pail 1000"]
["NA","RA-1588/4","For four 2 wire cables or combinations of 2, 3, and 4 wire cables stacked up to 11/16” high. "," 1/2”","White","Box 50"]
["NA","RA-1582/4",null," 1/2”","White","Pail 1000"]
["NA","RA-6250","5/8” STRAP FOR 10/2 NM AND UF CABLE, 14/3 UF CABLE, AND OTHER CABLE UP TO .625” WIDE","5/8\"","White","Box 100"]
["PS-175ZN","RA-1455P","Straps for Nonmetallic-Sheathed and Underground Feeder Cable (Continued) 3/4” STRAP FOR 2 WIRE NM AND UF CABLE UP TO NO. 8, 3 WIRE UF CABLE UP TO NO. 12, AND OTHER CABLE UP TO .750” WIDE.  ","3/4\"","White","Bag 1000"]
["PS-175","RA-1555",null,"3/4\"","White","Box 100"]
["PS-175","RA-1560",null,"3/4\"","White","Bulk 5000"]
["PS-175","RA-1562",null,"3/4\"","White","Pail 1500"]
["PS-175","RA-1566",null,"3/4\"","White","Bag 5000"]
["NA","RA-1566UV",null,"3/4\"","Black","Bag 250"]
[null,null,"STRAPS FOR 3 AND 4 WIRE NM CABLE"]
["NA","RA-1610R","For 14/3, 12/3, and 14/4 NM Cable and other cable up to 5/16” Dia. ",".312\"","White","Box 100"]
["NA","RA-1620R","For 10/3 and 12/4 NM Cable and other cable up to 13/32” Dia. ",".406\"","White","Box 100"]
["NA","RA-1630R","For 8/3 NM Cable and other cable up to 1/2” Dia. ",".500\"","White","Box 100"]
["NA","RA-1640R","For 6/3 NM Cable and other cable up to 9/16\" Dia.",".563\"","White","Box 50"]
["NA","RA-1650R","For other round cable and tubing up to 5/8” Dia.",".625\"","White","Box 50"]
[null,null,"STRAPS FOR UF CABLE - The standard color is gray with a UV stabilizer. For prolonged outdoor exposure, black colored straps with a UV stabilizer are also available."]
["NA","UF-2040","For 8/3 UF Cable. ",".336\" x 1.077\"","Gray","Box 50"]
["NA","UF-2050","For 6/3 UF Cable.",".400\" x 1.300\"","Gray","Box 50"]
[null,null,"Straps for Armored Cable (AC) and Metal-Clad (MC) Cable"]
["NA","ACMC-10","For AC and MC Cable from 3/8” (.375) to 1/2” (.500) Dia. ","1/2\"","Gray","Box 50"]
["NA","ACMC-20","For AC and MC Cable from 1/2” (.500) to 5/8” (.625) Dia.","5/8\"","Gray","Box 50"]
[null,null,"Straps for Service Entrance Cable and EMT"]
["GSE-515","RA-1710","For #6 SER (4 Conductor) and 1/2” EMT. ",".718\"","Gray","Box 50"]
["GSE-314","RA-1720","For #2 SER (4 Conductor) and 3/4” EMT. ",".937\"","Gray","Box 25"]
["NA","RA-1724","For #1/0 SER (4 Conductor). ","1.062\"","Gray","Box 25"]
["NA","RA-1730","For #2/0 SER (4 Conductor) and 1” EMT. ","1.160\"","Gray","Box 25"]
["NA","RA-1740","For #4/0 SER (4 Conductor). ","1.438\"","Gray","Box 10"]
["GSE-115","RA-1750","For #6 SEU (3 Conductor)",".437\" x .750\"","Gray","Box 100"]
["GSE-215","RA-1760","For #2 SEU (3 Conductor)",".550” x .972”","Gray","Box 50"]
["NA","RA-1765","For #2/0 SEU (3 Conductor)",".775” x 1.265”","Gray","Box 25"]
["GSE-402","RA-1770","For #4/0 SEU (3 Conductor)",".855” x 1.500”","Gray","Box 25"]
["GCC-120","PC-1210","2-Hole Straps for Plastic Pipe and Conduit","1/2” / .840”","Gray","Box 50"]
["GCC-220","PC-1220",null,"3/4” / 1.050”","Gray","Box 50"]
["GCC-310","PC-1230",null,"1” / 1.312”","Gray","Box 25"]
["GCC-410","PC-1240",null,"1-1/4” / 1.670” ","Gray","Box 25"]
[null,null,"Straps for Communication (CM) and Multipurpose (MP) Cable (Voice, Data, Instrumentation, Control, Alarm, Security and Audio Systems)"]
["NA","RA-1599","For Bell & Thermostat Wire and other CM and MP Cable up to 1/4” wide (2-Nail) "," .125” x .250”","Tan","Box 100"]
["NA","CM-140","For #12 Ground Wire, 22/4 Telephone Cable and other CM and MP Cable",".140”","Gray","Box 100"]
["NA","CM-180","For CM and MP Cable up to .180” Dia.",".180”","Ivory","Box 100"]
["PTP-100","CM-200","For Cat 5 and 5E 4 Pair CMP (Plenum) Cable and other CM and MP Cable",".200”","Blue","Box 100"]
["NA","CM-230","For Cat 5 and 5E 4 Pair CMR (Riser) and Cat 6 4 Pair CMP (Plenum) Cable and other CM and MP Cable",".230”","Black","Box 100"]
["NA","CM-240","For 6 Pair Telephone Cable, Cat 6 4 Pair CMR (Riser) Cable and other CM and MP Cable",".240”","Tan","Box 100"]
["NA","CM-25/50","For Hybrid Cable with (1) Cat 5E and (1) RG6 Quad",".250” x .500”","Black","Box 100"]
["NA","CM-275","For CM and MP Cable up to .275” Dia.",".275”","Black","Box 100"]
["NA","CM-300","For CM and MP Cable up to .300” Dia.",".300”","Black","Box 100"]
["PSG-50","CM-420","For 25 Pair Telephone Cable and other CM and MP Cable",".420”","Gray","Box 50"]
["NA","CM-640","For Hybrid Cable with (2) Cat 5E and (2) RG6 Quad",".640”","Blue","Box 50"]
[null,null,"Straps for Coaxial Cable - Our UV stabilized black straps are recommended for extended outdoor use. 1” nails are heat treated for use in wood, mortar joints, A ‘snap on’ feature for straps with the #8 Tapping Screw speeds installation.Hex Head Type AB Tapping Screw are also available. Type AB screws will cut threads in a pre-drilled hole in concrete, block, or any masonry or ‘soft’ masonry. Longer 1-3/16” heat treated nails. CC-1021 has a special 5/8” nail designed exclusively for use in masonry. To prevent cable damage from an accidental hammer blow, we offer straps with a #6 x 1” Phillips Head self-tapping screw. If used with a plastic screw anchor, this strap can also be used on masonry. Our CC-1006 strap has a #8 x 3/4” Type AB Tapping Screw for attaching #14 and #12 ground wire. Straps with a #8 x 1” Slotted/Phillips material."]
["NA","CC-1005","Hardnened Nail","#12 Ground Wire .140”","Black","Box 100"]
["NA","CC-1006","Head Type AB Tapping Screw ","#14 and #12 Ground Wire .110” - .145”","Black ","Box 50"]
["PCS-100","CC-1010","RG59 Hardened Nail ",".242”","Black","Box 100"]
["PEC-31525","CC-1012 ","RG59 Self-Tapping Screw ",".242”","Black","Box 100"]
["PEC-31525","CC-1016","RG59 Head Type AB Tapping Screw ",".242”","Black","Box 100"]
["PDC-1525BT","CC-2010","RG59 Dual Hardened Nail ",".250” x .500”","Black","Box 100"]
["PCS-100","CC-1020","RG6 Hardened Nail ",".275”","Black","Box 100"]
["PCS-100","CC-1021","RG6 Hardened Nail ",".275”","Black","Box 100"]
["NA","CC-1022","RG6 Self-Tapping Screw ",".275”","Black","Box 100"]
["NA","CC-1026 ","RG6 Head Type AB Self-Tapping Screw ",".275”","Black","Box 100"]
["PDC-1525BT","CC-2020","RG6 Dual Hardened Nail ",".305” x .594”","Black","Box 100"]
["NA","CC-2022","RG6 Self-Tapping Screw ",".305” x .594”","Black","Box 50"]
["NA","CC-2026","RG6 Head Type AB Self-Tapping Screw ",".305” x .594”","Black","Box 50"]
["PDC-1525BT","CC-1030 ","RG6 Quad Hardened Nail ",".300”","Black","Box 100"]
["NA","CC-1032","RG6 Quad Self-Tapping Screw ",".300”","Black","Box 100"]
["NA","CC-1036","RG6 Quad Head Type AB Tapping Screw ",".300”","Black","Box 100"]
["PTP-100M","CC-1060","RG11 Hardened Nail ",".395”","Black","Box 100"]
["PCS-3600","CC-1062","RG11 Self-Tapping Screw",".395”","Black","Box 100"]
["PCS-3600","CC-1066","RG11 Head Type AB Tapping Screw",".395”","Black","Box 100"]
[null,null,"Adjustable Coaxial Strap fits both RG6 and RG6 Quad Coaxial Cable. The unique wedge design of this strap enables it to adjust to the cable diameter as the screw is tightened."]
["NA","ACS-60","RG6 to RG6 Quad AB Tapping Screw",".275”","Black","Box 50"]
["NA","ACS-61","RG6 to RG6 Quad AB Tapping Screw",".275”","Black","Pail 1000"]
[null,null,"Straps for Plastic and Copper Tubing"]
["NA","WA-1810","For 1/2” Plastic and Copper Tubing",".625”","Tan","Box 100"]
["NA","WA-1820","For 3/4” Plastic and Copper Tubing",".875”","Tan","Box 25"]
[null,null,"Straps for PEX and Copper Tubing"]
["NA","PEX-50R","For 1/2” PEX Tubing",".625”","Red","Box 100"]
["NA","PEX-50B",null,".625”","Blue","Box 100"]
["NA","PEX-50W",null,".625”","White","Box 100"]
["NA","PEX-75R"," For 3/4” PEX Tubing",".875\"","Red","Box 50"]
["NA","PEX-75B",null,".875\"","Blue","Box 50"]
["NA","PEX-75W",null,".875\"","White","Box 50"]
["NA","PEX-100R","For 1” PEX Tubing","1.125\"","Red","Box 25"]
["NA","PEX-100B",null,"1.125\"","Blue","Box 25"]
["NA","PEX-100W",null,"1.125\"","White","Box 25"]

{"sheet":"Ideal","index":7,"n_rows":40,"n_cols":4,"rows_kept":40,"flags":["formulas_cached_only"]}
["GB","Cross","Discription","Quantity"]
["MCS-20W","BPSTCKR-15","Cable Stacker","Pack of 15"]
["MSB-1540",772840,"Brown Fiber","Pack of 40"]
["MSW-1540",772841,"White Fiber","Pack of 40"]
["PSW-1600T",772804,"3/16\" Sound Straps White","Pack of 25"]
["PSW-160",772805,"3/16\" Sound Straps White","Pack of 25"]
["PSB-1600T",772810,"3/16\" Sound Straps Black","Pack of 100"]
["PSB-160",772812,"3/16\" Sound Straps Black","Pack of 100"]
["PSB-1650T",772806,"1/4\" Coax Staple Black","Pack of 25"]
["PSB-100",772807,"1/4\" Coax Staple Black","Pack of 100"]
["PSW-1650T",772808,"1/4\" Coax Staple White","Pack of 25"]
["PSW-100",772809,"1/4\" Coax Staple White","Pack of 100"]
["GSE-515","BSER6-50","#6 SER and 1/2 in. EMT conduit","Pack of 50"]
["GSE-115","BSEU6-50","#6 and #8 SEU","Pack of 50"]
["GSE-330","BSER2-25","#2 SER and 3/4 in. EMT conduit","Pack of 25"]
["GSE-250","BSEU2-25","#2 SEU","Pack of 25"]
["GSE-402","BSER4/0-5","4/0 SEU and SER","Pack of 50"]
["NA","BMSE150-1","1-5/16\" x 3/4\"","Pack of 100"]
["NA","BMSE175-1","1-1/2\" x 1-1/16\"","Pack of 100"]
["NA",77280,"1/2 Plastic","Pack of 15"]
["PS-50",772801,"1/2 Plastic","Pack of 50"]
["PS-225J","BPS2-JR","1/2 Plastic","Jar 200"]
["NA","BPS2B-JR","1/2 Plastic","Jar 400"]
["PS-550","BPS2-5","1/2 Plastic","Pack of 500"]
["PS-750B","BPS2-5M","1/2 Plastic","Bucket 5k"]
["PS-1575T2",772802,"3/4\" Plastic","Pack of 15"]
["PS-75",772803,"3/4\" Plastic","Pack of 50"]
["PS-275N","BPS3-2","3/4\" Plastic","Pack of 250"]
["MSI-1525T",772816,"1/2\" Carbon Steel","Pack of 25"]
["MSI-50B",772817,"1/2\" Carbon Steel","Pack of 50"]
["MSI-150","BCS1-1","1/2\" Carbon Steel","Pack of 100"]
["MSI-200JT","BCS1-JR","1/2\" Carbon Steel","Jar 500"]
["MSI-550","BCS1-5","1/2\" Carbon Steel","Pack of 500"]
["MSI-950B","BCS1-5M","1/2\" Carbon Steel","Bucket 5k"]
["MSI-1575",772818,"9/16\" Carbon Steel","Pack of 25"]
["MSI-75",772819,"9/16\" Carbon Steel","Pack of 50"]
["NA","BCS2-1","9/16\" Carbon Steel","Pack of 100"]
["NA","BCS2-JR","9/16\" Carbon Steel","Jar 400"]
["NA","BCS2-5","9/16\" Carbon Steel","Pack of 500"]
["NA","BCS2-5M","9/16\" Carbon Steel","Bucket 5k"]

{"sheet":"Wireline","index":8,"n_rows":10,"n_cols":3,"rows_kept":10,"flags":["formulas_cached_only"]}
["GB","Wireline","Description"]
["PS-550",12550,"1/2 ROMX STPL (500/BAG)"]
["PS-750B",12576,"2000CT BUCKET 1/2 ROMX STPL"]
["PS-275N",34550,"3/4 ROMX STPL (250/BAG)"]
["GSE-515",41150,"#6 SER STPL (50/BAG)"]
["GSE-330",43125,"#2 SER STPL (25/BAG)"]
["NA",46125,"4/0 SER STPL (25/BAG)"]
["NA",47125,"2/0 SER STPL (25/BAG)"]
["NA",71125,"8/3 ROMEX STAPLE (25/BAG)"]
["NA",72125,"6/3 ROMEX STAPLE (25/BAG)"]

{"sheet":"Viking","index":9,"n_rows":116,"n_cols":8,"rows_kept":116,"merged":[[0,0,2,0],[0,3,2,3],[17,3,20,3],[19,1,20,1],[19,2,20,2],[19,4,20,4],[19,6,20,6],[19,7,20,7],[21,3,24,3],[23,1,24,1],[23,2,24,2],[23,4,24,4],[23,6,24,6],[23,7,24,7],[25,3,28,3],[27,0,28,0],[27,1,28,1],[27,2,28,2],[27,4,28,4],[27,6,28,6],[27,7,28,7],[53,0,55,0],[53,1,55,1],[53,2,55,2],[53,4,55,4],[53,5,55,5],[53,6,55,6],[53,7,55,7],[58,0,60,0],[58,1,60,1],[58,2,60,2],[58,4,60,4],[58,5,60,5],[58,6,60,6],[58,7,60,7],[63,0,64,0],[63,2,64,2],[63,3,64,3],[63,5,64,5],[63,6,64,6],[63,7,64,7],[65,0,66,0],[65,2,66,2],[65,3,66,3],[65,4,66,4],[65,5,66,5],[65,6,66,6],[65,7,66,7],[67,0,68,0],[67,2,68,2],[67,3,68,3],[67,5,68,5],[67,6,68,6],[67,7,68,7],[69,0,70,0],[69,2,70,2],[69,3,70,3],[69,4,70,4],[69,5,70,5],[69,6,70,6],[69,7,70,7],[71,0,72,0],[71,2,72,2],[71,3,72,3],[71,5,72,5],[71,6,72,6],[71,7,72,7],[73,0,74,0],[73,2,74,2],[73,3,74,3],[73,4,74,4],[73,5,74,5],[73,6,74,6],[73,7,74,7],[75,0,76,0],[75,2,76,2],[75,3,76,3],[75,5,76,5],[75,6,76,6],[75,7,76,7],[77,0,79,0],[77,2,79,2],[77,3,79,3],[77,4,79,4],[77,5,79,5],[77,6,79,6],[77,7,79,7],[80,0,81,0],[80,2,81,2],[80,3,81,3],[80,5,81,5],[80,6,81,6],[80,7,81,7],[82,0,83,0],[82,2,83,2],[82,3,83,3],[82,4,83,4],[82,5,83,5],[82,6,83,6],[82,7,83,7],[84,0,85,0],[84,2,85,2],[84,3,85,3],[84,5,85,5],[84,6,85,6],[84,7,85,7],[86,0,87,0],[86,2,87,2],[86,3,87,3],[86,4,87,4],[86,5,87,5],[86,6,87,6],[86,7,87,7],[88,0,89,0],[88,2,89,2],[88,3,89,3],[88,5,89,5],[88,6,89,6],[88,7,89,7],[90,0,91,0],[90,2,91,2],[90,3,91,3],[90,4,91,4],[90,5,91,5],[90,6,91,6],[90,7,91,7],[92,0,94,0],[92,2,94,2],[92,3,94,3],[92,5,94,5],[92,6,94,6],[92,7,94,7],[95,0,97,0],[95,2,97,2],[95,3,97,3],[95,4,97,4],[95,5,97,5],[95,6,97,6],[95,7,97,7],[98,0,99,0],[98,2,99,2],[98,3,99,3],[98,5,99,5],[98,6,99,6],[98,7,99,7],[100,0,101,0],[100,2,101,2],[100,3,101,3],[100,4,101,4],[100,5,101,5],[100,6,101,6],[100,7,101,7]],"flags":["formulas_cached_only"]}
["GB Cross","Size and Pack ","NAED","Cable Size","Item","Unit/Type","Case","Approx."]
[null,"Number","Product",null,"Number","Quantity","Quantity","Weight in Lbs"]
[null,null,"Code"]
["NA","200 PP 5M",29117,"NMC","C702118","Plastic Pail",5000,18]
["NA","200 PB 5M",29114,"2 Conductor","C702100","Bulk",5000,18]
["NA","**200 P5",29113,"#12 & 14 Wire","C702050",500,5000,18]
["NA","200 P1",29111,"&","C702001",100,10000,36]
["NA","*200 PB 5M EG",69114,"2 Conductor WG","C702209","Bulk",5000,18]
["NA","*200 P5 EG",69113,null,"C702258",500,10000,36]
["NA","*200 P1 EG",69111,null,"C702159",100,10000,36]
["NA","225 PP 5M",29217,"3 Conductor","C702415","Plastic Pail",5000,28]
["NA","225 PB 5M",29214,"#14, 12 & 10","C702407","Bulk",5000,28]
["NA","225 P5",29213,null,"C702357",500,10000,56]
["NA","225 P1",29211,null,"C702308",100,10000,56]
["NA","*225 PB 5M",69214,null,"C702423","Bulk",5000,28]
["NA","*225 P5",69213,null,"C702506",500,10000,56]
["NA","*225 P1",69211,null,"C702456",100,10000,56]
["NA","131 P1",59310,"SER 6/3","C704254","Box 100",5000,47]
["NA","131 PB 500",59311,null,"C704255","Bulk 500",2500,24]
["NA","131 BP 20",59315,null,"C704269","Blister Pack",360,3.5]
["NA",{"$nulls":4},"20 Count"]
["NA","141 P1",59410,"SER 2/3","C704304","Box 100",5000,59]
["NA","141 PB 500",59412,null,"C704306","Bulk 500",2500,30]
["NA","141 BP 10",59415,null,"C704311","Blister Pack",520,6]
["NA",{"$nulls":4},"10 Count"]
["NA","151 P1",59510,"SER 4/0","C704396","Box 100",1000,39]
["NA","151 PB 150",59512,null,"C704397","Bulk 150",150,6]
["GSE-402","151 BP 10",59511,null,"C704400","Blister Pack",180,7]
[{"$nulls":5},"10 Count"]
["MS-975B","125 PP 5M",9215,"3 Conductor","C704122","Plastic Pail",5000,36]
["NA","125 PTB",9218,"#10,12 & 14","C704124","Toolbox",5000,36]
["NA","125 PB 5M",9214,"Wire","C704106","Bulk",5000,36]
["NA","**125 PP 2.0M",9216,null,"C704141","Baby Pail",2000,"15**"]
["NA","125 P5",9213,"12 x 10 Wire","C704029",500,5000,36]
["NA","125 CP 450",9217,null,"C704148","Clear Plastic - 450",7200,53]
["NA","125 P1",9211,"2 Cond. WG","C704071",100,5000,36]
["NA","125 BP 100",9222,null,"C704200","Blister Pack 100",1800,15]
["NA","*125 PB 5M EG",59214,null,"C704130","Bulk",5000,36]
["MS-575","*125 P5 EG",59213,null,"C704205",500,5000,36]
["MS-175","*125 P1 EG",59211,null,"C704155",100,5000,36]
["MS-1575T","*125 BP 20",9221,null,"C704195","Blister Pack 20",1040,9]
["MS-950B","100 PP 5M",9115,"NMC","C703736","Plastic Pail",5000,24]
["NA","100 PTB 5M",9118,"#12 & 14","C703738","Toolbox",5000,24]
["NA","100 PB 5M",9114,null,"C703702","Bulk",5000,23]
["NA","**100 PP 2.5M",9116,"2 Conductor","C703743","Baby Pail",2500,"12**"]
["NA","100CP 750",9117,null,"C703760","Clear Plastic - 750",12000,59]
["NA","100 P5",9113,null,"C703652",500,10000,45]
["MA-150","100 P1",9111,null,"C703603",100,10000,45]
["MA-150","100 BP 100",9126,null,"C703910","Blister Pack 100",1800,10]
["NA","*100 PB 5M EG",59114,null,"C703850","Bulk",5000,23]
["MS-550","*100 P5 EG",59113,null,"C703801",500,10000,45]
["NA","*100 P1 EG",59111,null,"C703751",100,10000,45]
["MA-1550T","*100 BP 25",9125,null,"C703900","Blister Pack 25",1300,6]
["NA","LL 100 PP 3M",59515,"NMC","C703523","Plastic Pail",3000,21]
[{"$nulls":3},"2 Conductor"]
[{"$nulls":3},"&"]
["MSI-1525XL","LL 100 P1",59511,"3 Conductor W/G","C703501",100,5000,35]
["NA","LL 141 PB",59411,"SER 2/3","C704305",200,1000,19]
["NA","LL 100 PP 3M",59515,"NMC","C703523","Plastic Pail",3000,21]
[{"$nulls":3},"2 Conductor"]
[{"$nulls":3},"&"]
["NA","LL 100 P1",59511,"3 Conductor W/G","C703501",100,5000,35]
["NA","LL 141 PB",59411,"SER 2/3","C704305",200,1000,19]
["NA","Viking 151",59520,"C708000","Blister Card",12,60,5]
[null,"SSEC BC 5",null,null,"5 Count"]
["NA","Viking 151",59524,"C708002","50 Bulk",1,50,4.5]
[null,"SSEC Bulk 50"]
["NA","Viking 151",59521,"C708007","Blister Card",12,48,5]
[null,"SSG151 BC4",null,null,"4 Count"]
["NA","Viking 151",59525,"C708009","50 Bulk",1,50,5]
[null,"SSG151 Bulk 50"]
["NA","Viking 141",59422,"C707014","Blister Pack",18,108,5]
[null,"SS141 LLPG BP6",null,null,"6 Count"]
["NA","Viking 141",59426,"C707016","100 Bulk",1,100,5]
[null,"SS141 LLPG Bulk 100"]
["NA","Viking 141",59421,"C707007","Blister Pack",18,180,6]
[null,"SS141 BC BP10",null,null,"10 Count"]
["NA","Viking 141",59425,"C707009","100 Bulk",1,100,3.5]
[null,"SS141 BC"]
[null,"Bulk 100"]
["NA","Viking 131",59320,"C706000","Blister Pack ",18,180,3]
[null,"SSR131 BP10",null,null,"10 Count"]
["NA","Viking 131",59325,"C706029","200 Bulk",1,200,3]
[null,"SSR131 Bulk 20"]
["NA","Viking 131",59326,"C706030","Blister Pack",18,180,2.5]
[null,"SSR131 R12/14 BP10",null,null,"10 Count"]
["NA","Viking 131",59327,"C706031","200 Bulk",1,200,2.5]
[null,"SSR131 R12/14 Bulk 20"]
["NA","Viking 131",59323,"C706021","Blister Pack",18,180,4.5]
[null,"SSAC BP10",null,null,"10 Count"]
["NA","Viking 131",59326,"C706022","200 Bulk",1,200,4.5]
[null,"SSAC Bulk 200"]
["NA","Viking 131",59328,"C706032","Blister Pack",18,180,3]
[null,"SSR 131 R 14/3 Rnd",null,null,"10 Count"]
[null,"BP10"]
["NA","Viking 131",59329,"C706033","200 Bulk",1,200,3]
[null,"SSR 131 R 14/3"]
[null,"Bulk 200"]
["NA","Viking 131",59321,"C706007","Blister Pack",18,180,4]
[null,"SSC5 BP10",null,null,"10 Count"]
["NA","Viking 131",59325,"C706006","200 Bulk",1,200,4]
[null,"SSC5 Bulk 200"]
["NA","IN3125 PP 2.5M",9616,"NMC ","C702544","Plastic Pail",2500,21]
["NA","IN3125 PP 1.5M",9615,"#10,12 & 14","C702547","Plastic Pail",1500,13]
["NA","IN3125 CP 500",9611,null,"C702551","Clear Plastic",3000,26]
["MSI-75","IN3125 CP 175",9610,"3 Conductor","C702565","Clear Plastic",4200,36]
["MSI-1575","IN3125 BP 20",9617,null,"C702572","Blister Pack",360,3]
["MSI-950B","IN3000 PP 5M",9515,"NMC","C702500","Plastic Pail",5000,30]
["NA","IN3000 PB 5M",9514,"2 Cond.","C702507","Bulk",5000,30]
["NA","IN3000 PP 2.5M",9516,null,"C702523","Plastic Pail",2500,15]
["NA","IN3000 PTB 2.5M",9520,"#12 & 14","C702525","Toolbox",2500,15]
["NA","IN3000 CP800",9519,"Wire","C702541","Clear Plastic",3200,20]
["MSI-550","IN3000 P5",9513,null,"C702514",500,5000,30]
["NA","IN3000 CP300",9517,null,"C702537","Clear Plastic",7200,33]
["MSI-150","IN3000 P1",9511,null,"C702511",100,5000,30]
["MSI-1525T","IN3000 BP25",9518,null,"C702539","Blister Pack",450,3]

{"sheet":"Arrow","index":10,"n_rows":78,"n_cols":6,"rows_kept":78,"flags":["formulas_cached_only"]}
["GB","Arrow","Size","Pack Size","Insulated","Gun Style"]
["NA",186,"3/8\" (10mm)",1000,"No","Fits: T18 Stapler "]
["NA",187,"7/16\" (11mm)",1000,"No","Fits: T18 Stapler "]
["NA",205,"5/16\" (8mm)",1000,"No","Fits: T2025-6 Stapler "]
["NA",206,"3/8\" (10mm)",1000,"No","Fits: T2025-6 Stapler "]
["NA",208,"1/2\" (12mm)",1000,"No","Fits: T2025-6 Stapler "]
["NA",214,"1/4\" (6mm)",1000,"No","Fits: ES21, TT21, TT21K, JT21CM, JT27, & T27 Staplers "]
["NA",215,"5/16\" (8mm)",1000,"No","Fits: ES21, TT21, TT21K, JT21CM, JT27, & T27 Staplers "]
["NA",224,"1/4\" (6mm)",5000,"No","Fits: P22 Plier Stapler "]
["NA",225,"5/16\" (8mm)",5000,"No","Fits: P22 Plier Stapler "]
["NA",256,"3/8\" (10mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA",257,"7/16\" (11mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA",259,"9/16\" (14mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA",276,"3/8\" (10mm)",1000,"No","Fits: ES21, TT21, TT21K, JT21CM, JT27, & T27 Staplers "]
["NA",304,"1/4\" (6mm)",1000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA",305,"5/16\" (8mm)",1000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA",306,"3/8\" (10mm)",1000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA",354,"1/4\" (6mm)",5000,"No","Fits: P35 Plier Stapler "]
["NA",356,"3/8\" (10mm)",5000,"No","Fits: P35 Plier Stapler "]
["NA",376,"3/8\" (10mm)",1000,"No","Fits: T37 Stapler "]
["NA",378,"1/2\" (12mm)",1000,"No","Fits: T37 Stapler "]
["NA",379,"9/16\" (14mm)",1000,"No","Fits: T37 Stapler "]
["NA",759,"9/16\" (14mm)",1000,"No","Fits: T75 Stapler"]
["NA",2009,"9/16\" (14mm)",1000,"No","Fits: ET2025 "]
["NA",7510,"5/8\" (15mm)",1000,"No","T75 Stapler "]
["NA",7514,"7/8\" ",1000,"No","T75 Stapler "]
["NA",50424,"1/4\" (6mm)",1250,"No","Not Listed"]
["NA",50524,"5/16\" (8mm)",1250,"No","Not Listed"]
["NA",50624,"3/8\" (10mm)",1250,"No","Not Listed"]
["NA",50824,"1/2\" (12mm)",1250,"No","Not Listed"]
["NA",50924,"9/16\" (14mm)",1250,"No","Not Listed"]
["NA",591168,"1/4\"x1/4\" (6mmx6mm)",300,"Yes","Fits: T59 Stapler "]
["NA",591188,"1/4\"x5/16\" (6mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["NA",591189,"5/16\"x5/16\" (8mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["NA",721168,"13/64\"x31/64\" (5mmx12mm)",300,"Yes","Fits: T72 Stapler "]
["NA",721189,"11/32\"x18/32\" (8.7mmx15mm)",300,"Yes","Fits: T72 Stapler "]
["NA","186BE","3/8\" (10mm)",1000,"No","T18 Stapler "]
["NA","186M","3/8\" (10mm)",1000,"No","T18 Stapler "]
["NA","186MB","3/8\" (10mm)",1000,"No","T18 Stapler "]
["NA","187BE","7/16\" (11mm)",1000,"No","T18 Stapler "]
["NA","187M","7/16\" (11mm)",1000,"No","T18 Stapler "]
["NA","187MB","7/16\" (11mm)",1000,"No","T18 Stapler "]
["NA","256BE","3/8\" (10mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","256M","3/8\" (10mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","256MB","3/8\" (10mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","257BE","7/16\" (11mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","257M","7/16\" (11mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","257MB","7/16\" (11mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","259BE","9/16\" (14mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","259M","9/16\" (14mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","259MB","9/16\" (14mm)",1000,"No","Fits: T25, T25x, & T2025-6 Staplers "]
["NA","304IP","1/4\" (6mm)",5000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA","305IP","5/16\" (8mm)",5000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA","306IP","3/8\" (10mm)",5000,"No","Fits: T30 Stapler & HT30 Hammer Tacker "]
["NA","504IP","1/4\" (6mm)",5000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8000 "]
["NA","504MI","1/4\" (6mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8000 "]
["NA","504SS1","1/4\" (6mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8000 "]
["NA","505IP","5/16\" (8mm)",5000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8001 "]
["NA","505MI","5/16\" (8mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8002 "]
["NA","505SSI","5/16\" (8mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8003 "]
["NA","506IP","3/8\" (10mm)",5000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8004 "]
["NA","506MI","3/8\" (10mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8005 "]
["NA","506SSI","3/8\" (10mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8006 "]
["NA","508IP","1/2\" (12mm)",5000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8007 "]
["NA","508MI","1/2\" (12mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8008 "]
["NA","508SSI","1/2\" (12mm)",1000,"No","Fits: TT50, T50X, T50R.E.D., ET50R.E.D., T50ELITE, T50, T50PBN, ETF50BN, ET501, HT50, HT55, 5700, 8009 "]
["NA","50CT24","17/32\"",1250,"No","NA"]
["NA","591168BL","1/4\"x1/4\" (6mmx6mm)",300,"Yes","Fits: T59 Stapler "]
["NA","591188BL","1/4\"x5/16\" (6mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["NA","591188BLSS","1/4\"x5/16\" (6mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["MPS-2080","591189BL","5/16\"x5/16\" (8mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["MPS-2080","591189BLSS","5/16\"x5/16\" (8mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["MPS-2080","591189SS","5/16\"x5/16\" (8mmx8mm)",300,"Yes","Fits: T59 Stapler "]
["NA","721168HW","13/64\"x31/64\" (5mmx12mm)",300,"Yes","Fits: T72 Stapler "]
["NA","7510BE","5/8\" (15mm)",1000,"No","Fits: T75 Stapler "]
["NA","7510S","5/8\" (15mm)",1000,"No","Fits: T75 Stapler "]
["NA","7514S","7/8\" (22mm)",1000,"No","Fits: T75 Stapler "]
["NA","759M","9/16\" (14mm)",1000,"No","Fits: T75 Stapler "]